PART 1 - GENERAL

1.01 SECTION INCLUDES

1. Telephone Service Entrance Raceway.
2. Equipment and Terminal Backboards.

1.02 RELATED SECTIONS

1. Section 26 05 33.13 Conduit and Raceways.
2. Section 26 05 53 Supporting Devices.
3. Section 26 36 23 Electrical Identification.

1.03 QUALITY ASSURANCE

A. Telephone Utility Company: Verizon.

B. Install work in accordance with Telephone Utility Company's rules and regulations.

1.04 PROJECT RECORD DOCUMENTS

A. Submit record documents under provisions of Division 01.

B. Accurately record location of service entrance conduit and termination backboards.

PART 2 - PRODUCTS

2.01 TELEPHONE TERMINATION BACKBOARDS

A. Material: BC Plywood.

B. Size: 4 x 8 feet, 3/4 inch thick, painted gray with fire resistant paint on all sides, installed by this Contractor.

2.02 RACEWAYS

One-four inch (1-4”) conduit shall be provided and installed by this Contractor from Verizon’s point of entrance at the property line to the demark location within the Owners building.

PART 3 -EXECUTION

3.01 EXAMINATION

A. Verify that surfaces are ready to receive work.

B. Verify that field measurements are as shown on drawings.

C. Beginning of installation means installer accepts existing conditions.

3.02 INSTALLATION

1. Support raceways under the provisions of Section 26 05 53, Supporting Devices.

B. Install pullwire in each empty telephone conduit.

C. Extend existing service entrance conduit system from existing telephone closet to new main telephone/communication room. Retrieve conduit system from outside or extend existing system.

**END OF SECTION**